The cylinder is cleaned of dirt and carbon. The gasket surfaces are checked for flatness. The cylinder is then bored to a plug fit on a boring bore 90 degrees to the deck. The clearance is then honed to size. We then plateau the finish to ensure max performance and reliability. If it is a 2 stroke cylinder we chamfer the port windows. The cylinder is then washed with hot soapy water and dried.